

1.: Open LoadConfig(FB550 24SSOP)V3.exe



2.: Click the green arrow  open the file with suffix for BIN files

3: To be updated mouse into the host computer, not through extension cords and HUB

4：



When appear PASS, then plug the update mouse

If you do not need to update, turn off the software.